It is necessary to install the libUSB library for the board to function.

1. Hold Shift while Powering Down, and select advanced options.

2. Select Number 7 during reboot to temporarily allow installation of unsigned drivers.

3. Run the inf-wizard.exe and follow the instructions to install the driver.

4. Unplug all USB devices other than the Tiger board for easy selection.

5. Fill in NanoRiver Technologies on the Manufacturer field; all others are not relevant.

6. Now that the driver is installed, the Tigerboard shell GUI's should function properly.